


**UNINSTALL AND REMOVE ALL OLD VERSIONS OF THE SCT\_PORT.EXE PROGRAM BEFORE DOING THIS UPDATE – ONLY USE THE LASTEST INSTALL PROGRAM**


1. Press and Hold both the PUSH key (Channel Knob Push) and MENU key, and TURN ON THE RADIO and the screen will show “WARNING Boot Mode for Sct!!!”
2. Use the USB cable to connect radio and your PC
3. Run the **most current** **SetupSCT\_Port. msi** file provided in this update and install. 
4. Run SCT\_PORT Host Controller by Double Clicking on the Icon on your Desktop.
5. Follow the screen guides below to set the SCT\_Port Host Controller to update the Base Band:




Select Platform as SCT3258



Select Tools - Config






Choose the Com port for your PC



Select

SCT\_PORT > Flash Update





With the radio still turned on and the programming cable attached.

Click on Init Port to verify Com Port is active

Message Will Show = “Init Port Successful !!”

Click on Flash Update button to begin the Base Band Update to the radio.





The update is now complete.

**Unplug Radio Power Source to reboot radio**.

Reapply Power and Turn Radio back on.